|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| O.O. | ***16-08628*****16-00458** | MISO No | ***1-11079165*****1-10893070** | File No. | 240801 |
| **Abnormal Operating Condition:** | 115 kV Line GS21 (Selkirk G.S. – Brokenhead) 230 kV Line D13R (Dorsey – Rosser)  |
| **Effective Dates:** | 2016-07-05 from 1200 to 2016-07-05 at 2100 CST(2016-07-05 from 1200 to 2016-07-05 at 2100 EST) |
| **Standing Guide Reference:** | System Study as per L. Ruchkall |

|  |  |
| --- | --- |
| **Description of Work:** | GS21 – Forced outageD13R – Ratio changes at Rosser. Dorsey RCM Maintenance |





|  |  |
| --- | --- |
| **Special Instructions to MHEB Operator:** | **Export**:  If RTCA indicates that the loss SR3 will cause overloads on SG12, transfer from IESO may need to be curtailed. **Import**: If RTCA indicates that the loss F3M, ST6 or ST5 will cause overloads on WT34, transfer from IESO may need to be curtailed. |

|  |  |
| --- | --- |
| **MISO North RC Notes:** | MH\_ONT\_E (Export) SOL = 205 MWMH\_ONT\_W (Import) SOL = 140 MW |
|  |  |
| **Special Instructions:** | **TOI Extensions** - This TOI may be extended until 23:59, by performing the following steps.a) Verify system conditions to confirm there are no additional tie line facilities outages, or new internal MH outages.b) Review RTCA to confirm there are no new contingencies.c) Contact MISO to confirm there are no new outages, if there are no new outages provide notice to MISO that MH is extending the TOI.d) Extend the outage in COLAe) Update TLAP outage tablef) Provide notice to affected balancing authorities |

|  |  |  |  |
| --- | --- | --- | --- |
| **Prepared By:** | M. Edmunds | **Date:** | 2016 07 05 |

Copies to:

 SOSS, System Control Centre NSSS, System Control Centre

 GSSS, System Control Centre GSO, System Control Centre

 Operating Order Ontario IESO

 MISO – St. Paul MHEB OASIS

 File 240801