|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| O.O. | **N/A** | | MISO No. | **N/A** | File No. | 240801 |
| **Normal Operating Condition:** | | Up to 500 MW of TRM on the MHEX\_N interface is reserved for the delivery of CRSG. The CRSG release is reviewed weekly and is normally released at midnight for the next seven days.  Current Status: Release 500 MW of CRSG on MHEX\_N | | | | |
| **Effective Dates:** | | 2016-01-01 to 2016-12-31 | | | | |
| **Standing Guide Reference:** | | MHEX Standing Guide | | | | |

|  |  |
| --- | --- |
| **Special Instructions to MHEB Operator:** | A) Prior to releasing CRSG, Manitoba Hydro System Operators must ensure that sufficient generation reserves are available within the Manitoba Hydro System relative to the amount of CRSG to be released. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Prepared By:** | Scott Brooks | **Date:** | 2016 - 12 - 30 |

Copies to:

SOSS, System Control Centre NSSS, System Control Centre

GSSS, System Control Centre GSO, System Control Centre

MISO – St. Paul