|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| O.O. | **18-01986-OO** | | MISO No. | **1-17992117** | File No. | 240802 |
| **Name of Outage:** | | Cliff Lake 230-115 kV Bank 1 ***and,***  115 kV Line FC56 (Border - Cliff Lake) | | | | |
| **Effective Dates:** | | 2018-05-15 from 0800 to 2018-05-16 at 1600 CDT  (2018-05-15 from 0800 to 2018-05-16 at 1600 EST) | | | | |
| **Standing Guide Reference:** | | MH-SPCN Standing Guide | | | | |

|  |  |
| --- | --- |
| **System**  **Posturing** |  |
| **Description**  **of Work:** | Insulation testing on Cliff Lake Bank 1, protection mtce/trip tests. |



|  |  |
| --- | --- |
| **Special Notes to MISO North RC** |  |

|  |  |
| --- | --- |
| **Special Instructions to MHEB Operator:** |  |

|  |  |
| --- | --- |
| **Special Instructions** | **TOI Extensions** - This TOI may be extended until 23:59 by performing the following steps:   1. 1. Verify system conditions to confirm there are no additional tie line facilities outages, or new internal MH outages. 2. 2. Review RTCA to confirm there are no new contingencies. 3. 3. Contact MISO to confirm there are no new outages, if there are no new outages provide notice to MISO that MH is extending the TOI. 4. 4. Extend the outage in COLA. 5. 5. Update TLAP outage table.   6. Provide notice to affected balancing authorities. |

|  |  |  |  |
| --- | --- | --- | --- |
| **Prepared By:** | D. Williams | **Date:** | **2018.04.24** |

Copies to:

SPSO, System Control Centre NSSS, System Control Centre

GSSS, System Control Centre GSO, System Control Centre

Operating Order File 240802

MHEB OASIS MISO – St. Paul

SPC – Yong Zheng SPC - Colin Nicholson